> To Configure Quick Shifter
> The Quick Shifter accessory for the Power Commander V, when enabled and set-up, will kill engine power for a moment when the shift lever is actuated, allowing full throttle shifts without the clutch.

> 1 | Select Power Commander Tools >Configure >Feature Enables and Selection Inputs.

> 2 | Select the On/Off box to enable or disable Quick Shifter.

> 3 | Using the drop-down arrow, select which switch input will be used. For more information, refer to Power Commander V Switch Inputs.

> 4 | Click Configure to open the Quick Shifter Configuration window.

> 5 | Using the drop-down arrow, select a Mode.

> Single Time—uses the same shift kill time for all shifts.
> Gear Dependent—allows a different shift kill time for each gear change. Gear Dependent requires a gear indicator set-up. For more information, refer to To Calibrate the Gear Position.

> 6 | Using the drop-down arrow, select a Switch Style.

> In most cases the Power Commander V is configured correctly for the Switch Style.
> Normally Closed—use this setting for a Quick Shifter switch that is in the closed state at rest.
> Normally Open—use this setting for a Quick Shifter switch that is in the open state at rest.
> Contact Dynojet for more information.

> 7 | Enter a Minimum RPM.

> Below the Minimum RPM, the Quick Shift will not function.

> 8 | Enter a Shift Interval.

> The Shift Interval is the minimum time between each shift. If a second shift event occurs sooner than the length of time set here, it will be ignored.

> 9 | Enter the Shift Kill times.

> The Shift Kill Time is the amount of time (in milliseconds, 1000mS=1 second) that engine power will be cut for one shift event. If you selected Gear Dependent mode, set a shift kill time for each gear change.

> 10 | Using the drop-down arrow, select a Kill Mode.

> Kill Fuel Only—interrupts fuel delivery during Quick Shift (including the secondary fuel module, if connected).
> Kill Ignition Only—interrupts spark delivery during Quick Shift.
> Kill Fuel and Ignition—interrupts fuel delivery (including the secondary fuel module, if connected) and interrupts spark delivery during Quick Shift.

> 11 | Click OK to accept the changes.

> Or
> Click Cancel to close the window without changes.