> To Configure Rev X-Tend
> Some models of Power Commander V allow you to increase the maximum RPM above what the stock electronics allow.

> 1 | Select Power Commander Tools Configure Rev X-Tend.

> 2 | Select the Enabled box to enable or disable Rev X-Tend.

> 3 | Enter the Key in the Load Key text box.

> You will need a key to activate the Rev X-Tend feature. The key is available from your Dynojet salesman.

> 4 | Click Load Key.

> 5 | Click OK to accept the changes.

> Or
> Click Cancel to close the window without changes.