> To Configure Auto Tune
> Before you can configure Auto Tune, you will need an Auto Tune kit.
> Note: Map Switch and Auto Tune can not be enabled at the same time.

> 1 | Select Power Commander Tools >Configure >Feature Enables and Selection Inputs.

> 2 | Select the On/Off box to enable or disable Auto Tune.

> 3 | Click Configure to open the Auto Tune Configuration window.

> 4 | Enable or disable the Require Run Time.

> Minimum Run Time—is the length of time after startup before Auto Tune starts.

> 5 | Enable or disable the Require Engine Temp.

> Minimum Temp—Auto Tune will not start until this engine temperature is reached. Enter a temperature in Fahrenheit if Harley ECM Data is enabled and configured. For an analog temperature sensor, the units are dependent on the settings entered in the Engine Temperature tab.

> 6 | Enter the Trim Settings.

> The Max Enrichment Trim/Max Enleanment Trim—the maximum percentage of fuel changes Auto Tune will make during an Auto Tune session.

> 7 | Using the drop-down list, select the number of O2 sensors.

> 8 | Click OK to accept the changes.

> Or
> Click Cancel to exit the window with no changes.

> 9 | Click OK to accept the changes in the Feature Selections window.

> 10 | Click Yes to disable the map switch feature and enable Auto Tune.

> Note: Map Switch and Auto Tune can not be enabled at the same time.

> 11 | Click Yes to add Auto Tune tables.

> Note: The map position 2 tables will be replaced by Auto Tune tables. You cannot have map position 2 tables and Auto Tune tables at the same time.

> 12 | Select the device and style.

> Single Fuel Device—will Auto Tune only the primary fuel device.
> Both Fuel Devices—will Auto Tune both the primary fuel device (PCV) and the secondary fuel device (SFM).
> Throttle Position—will Auto Tune the %Throttle table.
> Pressure—will Auto Tune the Pressure table.
> Note: A pressure table must be configured to use this option. For more information, refer to To Add a Fuel Table (Pressure).