> To Configure the Pressure Input
> The Power Commander V has an analog voltage input. This input can be used with a 0-5V pressure sensor.

> 1 | Select Power Commander Tools >Configure >Pressure Input.

> 2 | Select the Enabled box.

> 3 | Using the drop-down arrow, choose the number of columns you wish to display.

> 4 | Using the information provided with your sensor, enter the voltages and display values.

> For example: 0.5V=0 psi, 4.5V=50 psi.

> 5 | Click OK to accept the changes.

> Or
> Click Cancel to close the window without changes.