> To Configure Map Switch
> The map switch allows you to switch between two different maps within the Power Commander V.

> 1 | Select Power Commander Tools >Configure >Feature Enables and Selection Inputs.

> 2 | Select the On/Off box to enable or disable Map Switch.

> Note: Map Switch can be used for multiple maps or to turn Auto Tune on/off; however, you cannot use it for both.

> 3 | Using the drop-down arrow, select which switch input will be used. For more information, refer to Power Commander V Switch Inputs.

> 4 | Click OK to accept the changes.

> Or
> Click Cancel to close the window without changes.

> 5 | Once Map Switch is enabled, click Send Map.

> 6 | Click Position 1. This will send the map to position 1.

> 7 | To send a map to position 2, click Send Map, and select Position 2.

> This will send the same map to position 2. You can modify this map and send the modified map to position 2.
> Or
> Modify the map on the screen, click Send Map, and select Position 2.