> To Calibrate the Speed
> Speed calibration should be performed on a dyno. There are two methods for calibrating speed.
> Speed Calibration Method 1

> 1 | Select Power Commander Tools Calibrate Speed Input.

> 2 | Verify the engine is running.

> 3 | Type in a Target Speed.

> 4 | Hold the bike at the target speed. It does not matter which gear you are in.

> 5 | Click Calibrate.

> 6 | Click OK.

> Speed Calibration Method 2
> Manually type in a scalar appropriate for your bike. Check with Dynojet technical support for these values.