> To Enable Auto Tune Switch
> When selected, Auto Tune will not start until the switch on the handle bar is toggled.

> 1 | Select Power Commander Tools >Configure >Feature Enables and Input Selections.

> 2 | Select the On/Off box to enable or disable Auto Tune Switch.

> 3 | Using the drop-down arrow, select which switch input will be used. For more information, refer to Power Commander V Switch Inputs.

> 4 | Click OK to accept the changes.

> Or
> Click Cancel to close the window without changes.