> To Calibrate the Throttle Position
> For fly-by-wire motorcycles, do not calibrate the full throttle position unless you are on a dynamometer.

> 1 | Select Power Commander Tools Calibrate Throttle Position.

> 2 | Verify the engine is running.

> 3 | With the throttle closed, click Reset.

> 4 | Fully open the throttle and close it. The open throttle value will be stored.

> The open and closed number can be changed manually to fine tune.

> 5 | Click OK.