> To Configure Quick Shifter
> The Quick Shifter accessory for the Power Commander V, when enabled and set-up, will kill engine power for a moment when the shift lever is actuated, allowing full throttle shifts without the clutch.

> 1 | Select Power Commander Tools Configure Quick Shifter.

> 2 | Select the Enabled box.

> 3 | Using the drop-down arrow, select a Mode.

> Single Time—uses the same shift kill time for all shifts.
> Gear Dependent—allows a different shift kill time for each gear change. Gear Dependent requires a gear indicator set-up. For more information, refer to To Calibrate the Gear Position.

> 4 | Enter a Minimum RPM.

> Below the Minimum RPM, the Quick Shift will not function.

> 5 | Enter a Shift Interval.

> The Shift Interval is the minimum time between each shift. If a second shift event occurs sooner than the length of time set here, it will be ignored.

> 6 | Enter the Shift Kill times.

> The Shift Kill Time is the amount of time (in milliseconds, 1000mS=1 second) that engine power will be cut for one shift event. If you selected Gear Dependent mode, set a shift kill time for each gear change.

> 7 | Click OK to accept the changes.

> Or
> Click Cancel to close the window without changes.