> To Edit the Advance/Demote Map
> The following steps apply for both Fuel and Ignition.

> 1 | Select Map Tools >Advance/Demote Map.

> 2 | Using the RPM Resolution drop-down list, choose 250 or 500.

> RPM Resolution adjusts the resolution of the RPM axis on the table(s).

> 3 | Using the Secondary Mapping Mode drop-down list, choose Basic or Advanced.

> Basic—a single fuel table for the PCV and SFM. The SFM fuel table cannot be edited independently from the PCV fuel table.
> Advanced—a separate fuel table for the PCV and SFM. Each of these tables can be edited independently.

> 4 | To Set the Fuel Tables (TPS), click here.

> Using the Fuel Tables drop-down list, choose Basic, Cylinder Advanced, Gear Advanced, or Cylinder and Gear Advanced.
> The Fuel Tables drop-down sets basic or advanced fuel tables.
> Basic—a single fuel table.
> Cylinder Advanced—a separate fuel table for each cylinder.
> Gear Advanced—a separate fuel table for each gear.
> Cylinder and Gear Advanced—for each gear there is a fuel table for each cylinder.
> Note: Speed and Gear Position must be calibrated for gear advanced tables to work properly.

> 5 | To Set the Fuel Tables (Pressure), click here.

> Note: You must add a pressure table before setting the Fuel Tables (Pressure). For more information, refer To Add a Fuel Table (Pressure) and To Configure the Pressure Table Axis.
> Using the Fuel Tables drop-down list, choose Basic, Cylinder Advanced, Gear Advanced, or Cylinder and Gear Advanced.
> The Fuel Tables drop-down sets basic or advanced fuel tables.
> Basic—a single fuel table.
> Cylinder Advanced—a separate fuel table for each cylinder.
> Gear Advanced—a separate fuel table for each gear.
> Cylinder and Gear Advanced—for each gear there is a fuel table for each cylinder.
> Note: Speed and Gear Position must be calibrated for gear advanced tables to work properly.

> 6 | To Set the Ignition Tables (TPS), click here.

> Using the Ignition Tables drop-down list, choose Basic, Cylinder Advanced, Gear Advanced, or Cylinder and Gear Advanced.
> The Ignition Tables drop-down sets basic or advanced ignition tables.
> Basic—a single ignition table.
> Cylinder Advanced—a separate ignition table for each cylinder.
> Gear Advanced—a separate ignition table for each gear.
> Cylinder and Gear Advanced—for each gear there is a ignition table for each cylinder.
> Note: Speed and Gear Position must be calibrated for gear advanced tables to work properly.
> Note: Not all power commanders will have the ignition option.

> 7 | To Set the Ignition Tables (Pressure), click here.

> Using the Ignition Tables drop-down list, choose Basic, Cylinder Advanced, Gear Advanced, or Cylinder and Gear Advanced.
> The Ignition Tables drop-down sets basic or advanced ignition tables.
> Basic—a single ignition table.
> Cylinder Advanced—a separate ignition table for each cylinder.
> Gear Advanced—a separate ignition table for each gear.
> Cylinder and Gear Advanced—for each gear there is a ignition table for each cylinder.
> Note: Speed and Gear Position must be calibrated for gear advanced tables to work properly.
> Note: Not all power commanders will have the ignition option.

> 8 | To set the Target AFR Tables, click here.

> Using the Target AFR Tables drop-down list, choose Basic, Cylinder Advanced, or Cylinder and Gear Advanced.
> The Target AFR Tables drop-down sets basic or advanced AFR tables.
> Basic—a single AFR table.
> Cylinder Advanced—a separate AFR table for each cylinder.
> Cylinder and Gear Advanced—for each gear there is an AFR table for each cylinder.

> 9 | To set the Auto Tune Method, click here.

> Using the Auto Tune Method drop-down list, choose PCV Only or PCV and SFM.
> PCV Only—Auto Tune makes a trim table for the PCV and will make changes to the PCV only.
> PCV and SFM—Auto Tune makes changes to the fuel table in both the PCV and SFM with a trim table for the PCV and a trim table for the SFM but only one target table.

> 10 | To set the Auto Tune Style, click here.

> TPS—standard Auto Tune mode is to tune throttle position and RPM.
> Pressure—select pressure if you have a pressure table and want Auto Tune to tune the pressure table.

> 11 | Click OK to accept your changes.

> Or
> Click Cancel to close the window with no changes.