> To Configure Accel Pump
> Accel Pump adds extra fuel when the throttle is moved quickly.
> Note: The vehicle’s fuel injection system will likely have some accel pump functionality. The PCV Accel Pump will be in addition to the existing vehicle’s accel pump functionality.

> 1 | Select Power Commander Tools >Configure >Feature Enables and Selection Inputs.

> 2 | Select the On/Off box to enable or disable Accel Pump.

> 3 | Click Configure to open the Accel Pump Configuration window.

> 4 | Enter a number between 0 and 100 in the Trigger (% Delta Throttle) field. This number represents the sensitivity of the accel pump event. With a smaller number, an accel pump event is more likely.

> Or
> Use the Capture feature to automatically fill in the Trigger field.

> 4a | Click Capture.

> 4b | Blip the throttle.

> 4c | Click OK to accept the changes.

> 5 | Enter the number of engine revolutions in the Duration field. This is the number of engine revolutions where fuel will be added by the PCV Accel Pump feature.

> 6 | Enter the percentage of fuel in the Fuel Adjustment (%) field. This is the percentage of fuel to be added during the accel pump event.

> 7 | Click OK to accept the changes.

> Or
> Click Cancel to close the window without changes.