> To Configure Harley ECM Data
> The Power Commander V monitors engine parameters from the on-board diagnostics (Harley Davidson only).

> 1 | Select Power Commander Tools Configure Harley ECM Data.

> 2 | Select the Diagnostic Port Enabled box to enable or disable Harley ECM Data.

> 3 | Select which channel you would like enabled.

> 4 | Click OK to accept the changes.

> Or
> Click Cancel to close the window without changes.