> To Configure Rev X-Tend
> Some models of Power Commander V allow you to increase the maximum RPM above what the stock electronics allow.
> If you have more than one module, you must sync the modules. For more information, refer To Configure the Sync Devices Utility.

> 1 | Select Power Commander Tools >Configure >Feature Enables and Selection Inputs.

> 2 | Select the On/Off box to enable or disable Rev X-tend.

> 3 | Click Configure to open the Rev X-tend Configuration window.

> 4 | Enter the Key in the Load Key text box.

> Before entering the key, all devices must be powered up either with a USB cable to each module or with the vehicle running.
> You will need a key to activate the Rev X-Tend feature. The key is available from your Dynojet salesman.

> 5 | Click Load Key.

> 6 | Click OK to accept the changes.

> Or
> Click Cancel to close the window without changes.