> To Configure In-Field Fuel Adjustments
> The Power Commander V combined with the Dynojet LCD Display allows you to make fueling changes in the field without a computer.
> The slider bars will show any changes made with the Dynojet LCD Display.

> 1 | Select Power Commander Tools >Configure >In-Field Fuel Adjustments.

> Note: The fuel changes made here apply to all throttle positions.

> 2 | Use the slider bars to make fueling changes. Any changes made in the software will override settings made using the LCD Display.

> 3 | Enter a number for the Low RPM and for the High RPM.

> Note: The RPM range between high and low is adjusted using the middle slider bar.

> 4 | Enter a number for the Slope. The default is 200.

> The slope sets the RPM span over which the fuel change will occur.

> 5 | Click Apply to accept the changes.

> Or
> Click Close to close the window without changes.