> To Calibrate the Gear Position
> Gear calibration should be performed on a dyno. There are two methods for calibrating gear.
> Note: Speed calibration must be completed and you must click OK before proceeding with gear calibration.
> Gear Calibration Method 1

> 1 | Select Power Commander Tools Calibrate Gear Position.

> 2 | Verify the engine is running.

> 3 | With the bike in first gear and while holding the throttle steady, click Calibrate for Gear 1.

> 4 | With the bike in second gear and while holding the throttle steady, click Calibrate for Gear 2.

> 5 | Continue this process through all of the gears.

> 6 | Click OK.

> 7 | Click Advanced to manually enter Gear Widths for each Gear Position.

> Note: Do not do this unless instructed by Dynojet to do so.
> Gear Calibration Method 2
> Manually type in a gear appropriate for your bike. Check with Dynojet technical support for these values.