> To Configure the Engine Temperature
> The Power Commander V monitors engine temperature by reading the temperature from the on-board diagnostics (Harley Davidson only), connecting to the vehicles temperature sensor, or installing your own temperature sensor. Engine Temperature can be used with certain features, such as Auto Tune and Startup Fuel.

> 1 | Select Power Commander Tools >Configure >Engine Temperature.

> 2 | To connect to the on-board diagnostics (Harley Davidson only), click here.

> 2a | Select the Enabled box.

> 2b | Using the drop-down list, select Harley ECM Data.

> 2c | Click OK to accept the changes.

> Or
> Click Cancel to close the window without changes.

> 3 | To connect to the vehicle’s temperature sensor or install a temperature sensor, click here.

> 3a | Select the Enabled box.

> 3b | Using the drop-down list, select Analog Voltage.

> Note: If you are using a pressure sensor, you will not be able to use a temperature sensor. The Power Commander V has only one analog input.

> 3c | Using the drop-down arrow, choose the number of columns you wish to display.

> 3d | Using the information provided with your sensor, enter the voltages and display values.

> For example: 0.5V=0 F, 4.5V=200 F.

> 3e | Click OK to accept the changes.

> Or
> Click Cancel to close the window without changes.