> Keyboard Shortcuts
> A description of the keyboard shortcuts follows:

> to | do the following
> Open Map File | Hold down CTRL and press O
> Save Map File | Hold down CTRL and press S
> View Device Information | Hold down CTRL and press I
> Hide Notes | Hold down CTRL and press N
> View the Environment Options | Hold down CTRL and press E
> Calibrate the Throttle Position | Hold down CTRL and press T
> Calibrate the Speed Input | Hold down CTRL+ALT and press S
> Calibrate the Gear Position | Hold down CTRL and press G
> Configure the Engine Temperature | Hold down CTRL+ALT and press E
> Configure the Pressure Input | Hold down CTRL+ALT and press P
> Configure the Map Switch | Hold down CTRL+ALT and press M
> Configure the Quick Shifter | Hold down CTRL+ALT and press Q
> Configure the Accel Pump | Hold down CTRL+ALT and press C
> Configure the Startup Fuel | Hold down CTRL+ALT and press F
> Configure the Rev X-Tend | Hold down CTRL+ALT and press X
> Configure the Auto Tune | Hold down CTRL+ALT and press A
> Configure the Harley ECM Data | Hold down CTRL+ALT and press J
> Update the Firmware | Hold down CTRL and press U
> Search for Devices to Add | Press F10
> View the Help | Press F1
> View the About | Press F11
> Send a Table | Press Insert or Press F6
> Send a Map | Press F5
> Get a Table | Press F8
> Get a Map | Press F7