> To Configure Launch Control
> When enabled, Launch Control will hold the bike at the chosen RPM regardless of the throttle position.
> An external switch is required to activate Launch Control.

> 1 | Select Power Commander Tools >Configure >Feature Enables and Selection Inputs.

> 2 | Select the On/Off box to enable or disable Launch Control.

> 3 | Using the drop-down arrow, select which switch input will be used. For more information, refer to Power Commander V Switch Inputs.

> 4 | Click Configure to open the Launch Control Configuration window.

> 5 | Enable or disable the Use Timer To Arm.

> When enabled, Launch Control will not engage until the amount of time entered in the Timer Amount text box has passed.

> 6 | Enter the time in the Timer Amount (sec) text box.

> 7 | Using the Activate Switch Style drop-down list, choose Normally Open or Normally Closed.

> Normally Closed—use this setting for a launch control switch that is in the closed state at rest.
> Normally Open—use this setting for a launch control switch that is in the open state at rest.
> Contact Dynojet for more information.

> 8 | Enter the RPM in the Launch RPM text box.

> 9 | Click OK to accept the changes.

> Or
> Click Cancel to close the window without changes.