> To Configure Startup Fuel
> The Power Commander V allows you to add or take out fuel upon engine startup.

> 1 | Select Power Commander Tools Configure Startup Fuel.

> 2 | To configure the startup fuel using Run Time, click here.

> 2a | Select the Enabled box.

> 2b | Using the Mode drop-down list, select Run Time.

> 2c | Enter the desired startup time in the Run Time field.

> 2d | Enter the desired amount of fuel adjustment in the Add Fuel field.

> 2e | Click OK to accept the changes.

> Or
> Click Cancel to close the window without changes.

> 3 | To configure the startup fuel using Engine Temperature, click here.

> 3a | Select the Enabled box.

> 3b | Using the Mode drop-down list, select Engine Temperature.

> 3c | Using the drop-down list, select the number of columns.

> 3d | Enter a temperature and a corresponding fuel adjustment in each column.

> Note: You must configure Engine Temperature before using the temperature option in Startup Fuel.

> 3e | Click OK to accept the changes.

> Or
> Click Cancel to close the window without changes.