> To Configure Startup Fuel
> The Power Commander V allows you to add or take out fuel upon engine startup.

> 1 | Select Power Commander Tools >Configure >Feature Enables and Selection Inputs.

> 2 | Select the On/Off box to enable or disable Startup Fuel.

> 3 | Click Configure to open the Start Fuel Configuration window.

> 4 | To configure the startup fuel using Run Time, click here.

> 4a | Verify startup fuel is enabled.

> 4b | Using the Mode drop-down list, select Run Time.

> 4c | Enter the desired startup time in the Run Time field.

> 4d | Enter the desired amount of fuel adjustment in the Add Fuel field.

> 4e | Click OK to accept the changes.

> Or
> Click Cancel to close the window without changes.

> 5 | To configure the startup fuel using Engine Temperature, click here.

> 5a | Verify startup fuel is enabled.

> 5b | Using the Mode drop-down list, select Engine Temperature.

> 5c | Using the drop-down list, select the number of columns.

> 5d | Enter a temperature and a corresponding fuel adjustment in each column.

> Note: You must configure Engine Temperature before using the temperature option in Startup Fuel.

> 5e | Click OK to accept the changes.

> Or
> Click Cancel to close the window without changes.