> To Accept All Trims
> Accept All Trims applies the trim values to the base fuel table(s). The values in the base fuel tables will change by the amount in the trim table and the trim table will then be cleared.
> Select Map Tools >Auto Tune Tables >Accept All Trims.
> Or
> Right-click on the table and select Accept Selected Trims.
> Note: You must click Send Map to apply your changes to the power commander.